STERILIZER LOG

DATE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ UNIT NUMBER (if indicated): \_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| TIME | OPERATOR BEGIN | **INSTRUMENT**  **TYPE(S)** | **TEMP REACHED** | **PRESSURE REACHED** | **AMOUNT**  **OF TIME** | **OPERATOR**  **END** | **CHEMICAL INDICATORS** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |
|  |  |  |  |  |  |  | **Yes/No** |

\*Chemical integrators or system printouts may be attached instead of recording temperature, pressure and time of treatment.

Sterilizer Cleaning and Maintenance Record

Location of Sterilizer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Year: \_\_\_\_\_\_\_\_\_\_\_

**Follow manufacturer’s recommendations for specific cleaning products to be utilized.**

**Allow unit to cool before beginning the cleaning process to prevent possibility of burns.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Jan** | **Feb** | **Mar** | **Apr** | **May** | **Jun** | **Jul** | **Aug** | **Sept** | **Oct** | **Nov** | **Dec** |
| 1. Clean internal and external surfaces with soft dry cloth and occasionally with cloth and mild soap. |  |  |  |  |  |  |  |  |  |  |  |  |
| 2. Drain reservoir and fill with clean distilled water |  |  |  |  |  |  |  |  |  |  |  |  |
| 3. Flush system according to manufacturer’s recommendations. |  |  |  |  |  |  |  |  |  |  |  |  |
| 4. Remove door gasket, dam gasket and gasket ring and clean. |  |  |  |  |  |  |  |  |  |  |  |  |
| 5. Remove trays, tray rack etc and wipe off with cleaner. |  |  |  |  |  |  |  |  |  |  |  |  |
| 6. Locate chamber filters and clean. Rinse filter with clean, distilled water. Reinstall filters. |  |  |  |  |  |  |  |  |  |  |  |  |
| 7. Reinstall trays, tray rack, etc. |  |  |  |  |  |  |  |  |  |  |  |  |
| 8. Fill reservoir with clean, distilled water. |  |  |  |  |  |  |  |  |  |  |  |  |
| 9. Check pressure relief valve according to manufacturer’s instruction. |  |  |  |  |  |  |  |  |  |  |  |  |

**Sterilizer Service Information:** (to be filled out by facility)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Date Service Requested** | **Sterilizer Model** | **Sterilizer Serial Number** | **Name of Person Requesting Service** | **Reason for Service Request** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

\*Attach invoice as proof of service performed